
SiS 7012 PCI Audio Driver Setup Readme File
-------------------------------------------

To install Windows 95/98/Me/NT4/Win2000/WinXP drivers, please run SETUP.EXE in this directory;
To uninstall Windows 95/98/Me/NT4/Win2000/WinXP drivers, please run Control_Panel->
Add/Remove_Program->SiS Audio Driver

To install drivers for other O.S, please see README file under each
driver directory.

SETUP.EXE Automatically installs WDM or VxD driver for Windows 95/98 base on
the O.S version:
  -WDM driver is installed for Windows 98SE and
  -VxD is installed for Windows 98OEM (first edition, 4.10.1998) and
Windows 95.  

To force installing VxD driver for Windows 98SE, please run
"SETUP.EXE -vxd" using Windows Start->Run


To update the driver, just run SETUP.EXE directly. SETUP will overwrite
the old driver with the current one.


Setup Switch Description
------------------------

You can run "Setup -sw" for desired operation. For example,
run "Setup -s" for silent installing driver.
Or add a line "CmdLine=-s" in the [Startup] section of file Setup.ini
then just run Setup without any switch.
The switches are

 -vxd
  force installing VxD driver on Windows 98SE;

 -ar
  install AudioRack;

 -s
  silent install, *NOTE* this switch should be put as the last one

Win2000/WinXP Setup Limitation
------------------------
Please do not use SILENT INSTALL after remove audio device. Please restart computer after remove audio device then doing silent install.



Play .mid file under NT4/VxD
-----------------------
-1.Download DLS or SF2 file from WWW
-2.Use SiSAudUt.exe for NT4 drivers to set it's midi sample file(DLS or SF2)
-3.If you want to change midi sample file, repeat step 1 and 2

